### header

### Hotels - Hardware Sets - Typical

## General Notes and guidelines for a complete Hardware schedule:

Where DHSI frame seals and door bottoms are specified for smoke, fire and sound, it is intended for all openings requiring Listed sealing products be the same manufacturer: DHSI

**Sample Finish shown, Consult DHSI for options**

**HW-1 GUEST ENTRY PART NUMBER FINISH MFG**

3 EA. HINGES AS SPECIFIED

1 EA. CLOSER AS SPECIFIED

1 EA. ELECTONIC CARD LOCKSET Section 08711

1 EA. DOOR VIEWER 190 DEGREE #DV 626 DHSI

1 EA. DOOR VIEWER COVER #DVC 626 DHSI

1 SET FRAME SEAL GASKET #105 “Cush ‘N’ Seal” DB DHSI

1 EA. MORTISE DOOR BOTTOM #AMDB4-4 X SWE DHSI

1 SET DECIBEL PLUGS #DP GY DHSI

1 EA. 3/4” high TRANSITION #CTT 2.75 Carpet-to-Tile DB DHSI

1 SET FRAME ALIGNMENT BRACKET #FA/SB – new frames only DHSI

See alternates below, including Low-Profile transition for 0” to 1/4” flooring

Submittal shall use only a DHSI architectural detail

1 EA. PRIVACY GUARD #SAL “Secur-A-Latch” 626 DHSI

1 EA. PRIVACY GUARD SCREW COVER #SAL-SC Screw Cover 626 DHSI

1 EA. DEADBOLT SILENCER #CNB “Cush N Bolt” 626 DHSI

NOTE: Provide 2 door viewers on H/C guest rooms.

NOTE: #FA/SB used with new frame installation only

**ALTERNATES:**

**HW-1 CAP SWEEP Door Bottom**

1 EA DOOR BOTTOM #CS-36 Cap Sweep with 1/2" fins DB DHSI

**HW-1 Flooring Transitions**  **Per flooring thickness and materials:**

1 EA. 3/4” high TRANSITION #TTT 2.75 Tile-to-Tile DB DHSI

1 EA. 3/4” high TRANSITION #FT 2.75 Carpet-to-Carpet DB DHSI

1 EA. 1/2” high **LOW PROFILE TRANSITION** #LP 2.75 Low Profile 0” to ¼” flooring DB DHSI

1 EA. GRANITE TRANSITION STONE, QUARTZ OR GRANITE By Others

**HW-1 AMU** **option for corridor air supply Suffix “AMU” available on all door bottoms:**

1 EA DOOR BOTTOM #CS.75 - 36 x AMU Cap Sweep DB DHSI

With 3/4" “AMU” option for airflow

1 EA. MORTISE DOOR BOTTOM #AMDB X SWE x AMU DHSI

With 3/4" “AMU” option for airflow

NOTE: PATENTED AMU OPTION Consult DHSI for profiles and CFM specifics

## HW-2 CONNECTING DOORS PART NUMBER FINISH MFG

6 EA. HINGES AS SPECIFIED

2 EA. CONNECTING ROOM LATCHSET AS SPECIFIED

2 EA. DEADLOCK AS SPECIFIED

2 EA. WALL STOP AS SPECIFIED

2 SETS FRAME SEAL GASKET #105 “Cush ‘N’ Seal” DB DHSI

2 EA. MORTISE DOOR BOTTOM #AMDB4-4 X SWE DHSI

2 SETS DECIBEL PLUGS #DP GY DHSI

1 EA 3/4” high TRANSITION, ADJUSTABLE #TTT-ADJ x frame depth DB DHSI

See alternates below, including Low-Profile transition for 0” to 1/4” flooring

Submittal shall use only a DHSI architectural detail

2 EA. PRIVACY GUARD #SAL “Secur-A-Latch” 626 DHSI

2 EA. PRIVACY GUARD SPACERS #SAL-CONN BK DHSI

2 EA. PRIVACY GUARD SCREW COVER #SAL-SC Screw Cover 626 DHSI

**ALTERNATES:**

**HW-2 CAP SWEEP Door Bottom**

2 EA DOOR BOTTOM #CS-36 Cap Sweep with 1/2" fins DB DHSI

**HW-2 Flooring Transitions**  **Per flooring thickness and materials:**

1 EA. 3/4” high TRANSITION, ADJUSTABLE #CTC-ADJ x frame depth DB DHSI

1 EA. 1/2” high **LOW PROFILE** TRANSITION, #LP-ADJ x frame depth DB DHSI

ADJUSTABLE

1 EA. GRANITE TRANSITION STONE, QUARTZ OR GRANITE By Others

## HW-6 STAIRWELL SINGLE PART NUMBER FINISH MFG

3 EA. HINGES AS SPECIFIED

1 EA. FIRE EXIT HDWE.-RIM AS SPECIFIED

1 EA. CLOSER AS SPECIFIED

1 SET FRAME SEAL GASKET #105 “Cush ‘N’ Seal” DB DHSI

1 EA. MORTISE DOOR BOTTOM #AMDB4-4 X SWE DHSI

1 SET DECIBEL PLUGS #DP GY DHSI

1 EA. 3/4" high TRANSITION #HS-CT 3.50 BLK DHSI

See alternates below, including Low-Profile transition for 0” to 1/4” flooring

Submittal shall use only a DHSI architectural detail

**ALTERNATES:**

**HW-6 CAP SWEEP Door Bottom**

1 EA DOOR BOTTOM #CS-36 Cap Sweep with 1/2" fins DB DHSI

**HW-6 Flooring Transitions**  **Per flooring thickness and materials:**

1 EA. 3/4” high TRANSITION #TTT 2.75 Tile-to-Tile DB DHSI

1 EA. 1/2” high **LOW PROFILE TRANSITION** #LP 2.75 Low Profile 0” to ¼” flooring DB DHSI

1 EA. GRANITE TRANSITION STONE, QUARTZ OR GRANITE By Others

## These are only typicals. Contact DHSI for full Hardware Sets for Cross-corridor, service, back of house, storage rooms, public bathroom, etc.

## Request DHSI architectural details for transition requirements such as carpet to tile, LVT to carpet tile, integral pad with standard carpet etc. Other options available for existing construction.

It is required that a distributor include the appropriate DHSI architectural details on a submittal. Sales cut sheets are not acceptable.

**Call DHSI to request a word document (.doc) version of the hardware sets for downloading or incorporating in your specs.**

08710 HOTELS – TYPICAL HW Sets-04 02-13-23